,Bowl Option##OTHER##,Tank Option##OTHER##,Model##OTHER##,Bowl Height##LENGTH##INCHES,Total Height##LENGTH##INCHES,Tank Position##LENGTH##INCHES,Product data url##OTHER##,Product Page URL##OTHER##,Product Documentation Link##OTHER##,Length##LENGTH##INCHES,Flush Rate##OTHER##,Distance to Drain##LENGTH##INCHES,Description##OTHER##
"22.0212 Bowl with 22.0300RWH Tank - 10"" Rough In",Bowl : 22.0212,Tank : 22.0300RWH,C22.011.01,15.5,30.75,16.1,https://www.bimobject.com/niagara/product/sabre1-10-gpf-10-rough-in-round-bowl-regular-height-toilet,https://pro.niagaracorp.com/product/sabre1-10-gpf-10-rough-in-round-bowl-regular-height-toilet/,https://pro.niagaracorp.com/wp-content/uploads/dlm_uploads/2021/04/Sabre_1.1_Round_10.pdf,27.4375,1.1 GPF,10,"SABRE™ with Stealth Technology® 1.1 GPF 10"" Rough-In Round Bowl Toilet"
"22.0212 Bowl with 22.0300LWH Tank - 10"" Rough In",Bowl : 22.0212,Tank : 22.0300LWH,C22.010.01,15.5,30.75,16.1,https://www.bimobject.com/niagara/product/sabre1-10-gpf-10-rough-in-round-bowl-regular-height-toilet,https://pro.niagaracorp.com/product/sabre1-10-gpf-10-rough-in-round-bowl-regular-height-toilet/,https://pro.niagaracorp.com/wp-content/uploads/dlm_uploads/2021/04/Sabre_1.1_Round_10.pdf,27.4375,1.1 GPF,10,"SABRE™ with Stealth Technology® 1.1 GPF 10"" Rough-In Round Bowl Toilet"
"22.0202 Bowl with 22.0300RWH Tank - 12"" Rough In",Bowl : 22.0202,Tank : 22.0300RWH,C22.001.01,15.5,30.75,16.1,https://www.bimobject.com/niagara/product/sabre1-10-gpf-12-rough-in-round-bowl-regular-height-toilet,https://pro.niagaracorp.com/product/sabre1-10-gpf-12-rough-in-round-bowl-regular-height-toilet/,https://pro.niagaracorp.com/wp-content/uploads/dlm_uploads/2021/04/Sabre_1.1_Round_12.pdf,27.4375,1.1 GPF,12,"SABRE™ with Stealth Technology® 1.1 GPF 12"" Rough-In Round Bowl Toilet"
"22.0202 Bowl with 22.0300LWH Tank - 12"" Rough In",Bowl : 22.0202,Tank : 22.0300LWH,C22.000.01,15.5,30.75,16.1,https://www.bimobject.com/niagara/product/sabre1-10-gpf-12-rough-in-round-bowl-regular-height-toilet,https://pro.niagaracorp.com/product/sabre1-10-gpf-12-rough-in-round-bowl-regular-height-toilet/,https://pro.niagaracorp.com/wp-content/uploads/dlm_uploads/2021/04/Sabre_1.1_Round_12.pdf,27.4375,1.1 GPF,12,"SABRE™ with Stealth Technology® 1.1 GPF 12"" Rough-In Round Bowl Toilet"
"22.0200 ADA Bowl with 22.0300RWH Tank - 12"" Rough In",Bowl : 22.0200,Tank : 22.0300RWH,C22.201.01,17,32.25,17.4375,https://www.bimobject.com/niagara/product/sabre1-10-gpf-12-rough-in-round-bowl-ada-height-toilet,https://pro.niagaracorp.com/product/sabre1-10-gpf-12-rough-in-round-bowl-ada-height-toilet/,https://pro.niagaracorp.com/wp-content/uploads/dlm_uploads/2021/04/Sabre_1.1_Round-ADA_12.pdf,27.4375,1.1 GPF,12,"SABRE™ with Stealth Technology® 1.1 GPF 12"" Rough-In Round Bowl ADA Height Toilet"
"22.0200 ADA Bowl with 22.0300LWH Tank - 12"" Rough In",Bowl : 22.0200,Tank : 22.0300LWH,C22.200.01,17,32.25,17.4375,https://www.bimobject.com/niagara/product/sabre1-10-gpf-12-rough-in-round-bowl-ada-height-toilet,https://pro.niagaracorp.com/product/sabre1-10-gpf-12-rough-in-round-bowl-ada-height-toilet/,https://pro.niagaracorp.com/wp-content/uploads/dlm_uploads/2021/04/Sabre_1.1_Round-ADA_12.pdf,27.4375,1.1 GPF,12,"SABRE™ with Stealth Technology® 1.1 GPF 12"" Rough-In Round Bowl ADA Height Toilet"
"22.0212 Bowl with 22.0301RWH Tank - 10"" Rough In",Bowl : 22.0212,Tank : 22.0301RWH,C22.013.01,15.5,30.75,16.1,https://www.bimobject.com/niagara/product/sabre1-28-gpf-10-rough-in-round-bowl-regular-height-toilet,https://pro.niagaracorp.com/product/sabre1-28-gpf-10-rough-in-round-bowl-regular-height-toilet/,https://pro.niagaracorp.com/wp-content/uploads/dlm_uploads/2021/04/Sabre_1.28_Round_10.pdf,27.4375,1.28 GPF,10,"SABRE™ with Stealth Technology® 1.28 GPF 10"" Rough-In Round Bowl Toilet"
"22.0212 Bowl with 22.0301LWH Tank - 10"" Rough In",Bowl : 22.0212,Tank : 22.0301LWH,C22.012.01,15.5,30.75,16.1,https://www.bimobject.com/niagara/product/sabre1-28-gpf-10-rough-in-round-bowl-regular-height-toilet,https://pro.niagaracorp.com/product/sabre1-28-gpf-10-rough-in-round-bowl-regular-height-toilet/,https://pro.niagaracorp.com/wp-content/uploads/dlm_uploads/2021/04/Sabre_1.28_Round_10.pdf,27.4375,1.28 GPF,10,"SABRE™ with Stealth Technology® 1.28 GPF 10"" Rough-In Round Bowl Toilet"
"22.0202 Bowl with 22.0301RWH Tank - 12"" Rough In",Bowl : 22.0202,Tank : 22.0301RWH,C22.003.01,15.5,30.75,16.1,https://www.bimobject.com/niagara/product/sabre1-28-gpf-12-rough-in-round-bowl-regular-height-toilet,https://pro.niagaracorp.com/product/sabre1-28-gpf-12-rough-in-round-bowl-regular-height-toilet/,https://pro.niagaracorp.com/wp-content/uploads/dlm_uploads/2021/04/Sabre_1.28_Round_12.pdf,27.4375,1.28 GPF,12,"SABRE™ with Stealth Technology® 1.28 GPF 12"" Rough-In Round Bowl Toilet"
"22.0202 Bowl with 22.0301LWH Tank - 12"" Rough In",Bowl : 22.0202,Tank : 22.0301LWH,C22.002.01,15.5,30.75,16.1,https://www.bimobject.com/niagara/product/sabre1-28-gpf-12-rough-in-round-bowl-regular-height-toilet,https://pro.niagaracorp.com/product/sabre1-28-gpf-12-rough-in-round-bowl-regular-height-toilet/,https://pro.niagaracorp.com/wp-content/uploads/dlm_uploads/2021/04/Sabre_1.28_Round_12.pdf,27.4375,1.28 GPF,12,"SABRE™ with Stealth Technology® 1.28 GPF 12"" Rough-In Round Bowl Toilet"
"22.0200 ADA Bowl with 22.0301RWH Tank - 12"" Rough In",Bowl : 22.0200,Tank : 22.0301RWH,C22.203.01,17,32.25,17.4375,https://www.bimobject.com/niagara/product/sabre1-28-gpf-12-rough-in-round-bowl-ada-height-toilet,https://pro.niagaracorp.com/product/sabre1-28-gpf-12-rough-in-round-bowl-ada-height-toilet/,https://pro.niagaracorp.com/wp-content/uploads/dlm_uploads/2021/04/Sabre_1.28_Round-ADA_12.pdf,27.4375,1.28 GPF,12,"SABRE™ with Stealth Technology® 1.28 GPF 12"" Rough-In Round Bowl ADA Height Toilet"
"22.0200 ADA Bowl with 22.0301LWH Tank - 12"" Rough In",Bowl : 22.0200,Tank : 22.0301LWH,C22.202.01,17,32.25,17.4375,https://www.bimobject.com/niagara/product/sabre1-28-gpf-12-rough-in-round-bowl-ada-height-toilet,https://pro.niagaracorp.com/product/sabre1-28-gpf-12-rough-in-round-bowl-ada-height-toilet/,https://pro.niagaracorp.com/wp-content/uploads/dlm_uploads/2021/04/Sabre_1.28_Round-ADA_12.pdf,27.4375,1.28 GPF,12,"SABRE™ with Stealth Technology® 1.28 GPF 12"" Rough-In Round Bowl ADA Height Toilet"
